
**468 KEY PRO third generation**


**Operating Instructions**

**operate steps:**

**1,Turn on the Left switch of 468 KEY PRO third generation, after turn on it, the main interface pops up. Then click “COPY”.**


**1贝46”**


**2,** **click “CMT46 collect” Upper left corner of the screen.**

****

**3,** **This page is a copy of the ID46-chip page, now it is copying ID46 chip.**

**3.1、Put the original chip vertically into the bottom right corner of the hole, click on " read UID". Note: Do not going to be flat on the hole nearby, this is not easy to read information inside the chip.**


****

**3.2、Put the new key vertically into the bottom right corner of the hole, click on "Conf ig". Note: Do not going to be flat on the hole nearby, this is not easy to read information inside the chip. **


**3.3、Use new car key collect information in car, first of all, take a key blank, put the new key into the key blank, insert the car key hole, four consecutive starts, each time interval of 3-5 seconds**

**.**


**3.4、Put the key which already collected information vertically into the bottom right corner of the hole, click on " read". Screen will appear a set of "random number" and "signature".**

****

**4, After crack Original key , put the original key hole vertically into the bottom right corner, click on " crack", the screen will display the progress of the original key crack.**



**5,New key copy. Put the key which already collected information vertically into the bottom right corner of the hole, click on “Copy”.** **Screen will display "copy successful" message.**

****

**6、If in the process, chip key copy failed, put the key into bottom right corner of the hole, click on "Initialize", restart again from the first step.**

